Linux kernel

ls /lib/modules/$(uname -r) build modules.alias modules.builtin modules.dep modules.devname modules.softdep modules.symbols.bin kernel modules.alias.bin modules.builtin.bin modules.dep.bin modules.order modules.symbols source

Драйверы

$ ls /lib/modules/$(uname -r)/kernel/drivers/ acpi bluetooth dax firewire hv infiniband media mmc nvme platform scsi thermal uwb w1 ata cdrom dca firmware hwmon input memstick mtd nvmem power spi thunderbolt vfio watchdog atm char devfreq gpio hwtracing isdn message net parport powercap ssb tty vhost xen bcma cpufreq dma gpu i2c leds mfd nfc pci pps staging uio video block crypto edac hid iio md misc nvdimm pcmcia ptp target usb virtio

Описание драйвера

$ modinfo acpi filename: /lib/modules/4.11.0-2-amd64/kernel/drivers/cpufreq/acpi-cpufreq.ko alias: acpi license: GPL description: ACPI Processor P-States Driver author: Paul Diefenbaugh, Dominik Brodowski alias: cpu:type:x86,ven*fam*mod*:feature:*00E8* alias: cpu:type:x86,ven*fam*mod*:feature:*0016* alias: acpi*:ACPI0007:* alias: acpi*:LNXCPU:* depends: intree: Y vermagic: 4.11.0-2-amd64 SMP mod_unload modversions parm: acpi_pstate_strict:value 0 or non-zero. non-zero -> strict ACPI checks are performed during frequency changes. (uint)

Загрузка драйвера

$ modprobe foo